{"text_format":"3","workbook":"xls","n_sheets":5,"sheets":["Sensor Data","Hg Sump Level","Temperatures","Hydraulic Pressure","Hg Vapor Levels"],"not_rendered":{"charts":4,"macros":1,"external_links":1},"unopened":[{"sheet":"Hg Sump Level","index":1,"reason":"not_a_worksheet"},{"sheet":"Temperatures","index":2,"reason":"not_a_worksheet"},{"sheet":"Hydraulic Pressure","index":3,"reason":"not_a_worksheet"},{"sheet":"Hg Vapor Levels","index":4,"reason":"not_a_worksheet"}],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sensor Data","index":0,"n_rows":10,"n_cols":14,"rows_kept":10,"flags":["formulas_cached_only"]}
["Log File Sensor Data"]
[]
[]
[]
["Timestamp","Hg Sump Level","Hg Temp","Hydraulic Fluid Temp","Hg Cylinder Inlet Temp","Secondary Air Temp","Downbeam Primary Window Temp","Downbeam Bore Temp","Upbeam Bore Temp","Nozzle Flange Temp","Hg Vapor 1","Hg Vapor 2","Port A Pressure","Port B Pressure"]
[null,"(cm)","(°C)","(°C)","(°C)","(°C)","(°C)","(°C)","(°C)","(°C)","(mg/m^3)","(mg/m^3)","(bar)","(bar)"]
["2006-11-30T18:01:04",9.2,{"v":24,"d":"24.0"},{"v":41,"d":"41.0"},{"v":26,"d":"26.0"},{"v":27,"d":"27.0"},{"v":28,"d":"28.0"},{"v":29,"d":"29.0"},{"v":32,"d":"32.0"},{"v":31,"d":"31.0"},0.017,0.005,0.1,0.4]
["2006-11-30T18:02:04",9.1,{"v":24,"d":"24.0"},{"v":41,"d":"41.0"},{"v":26,"d":"26.0"},{"v":27,"d":"27.0"},{"v":28,"d":"28.0"},{"v":29,"d":"29.0"},{"v":32,"d":"32.0"},{"v":31,"d":"31.0"},0.018,0.005,0.2,0.5]
["2006-11-30T18:03:04",{"v":9,"d":"9.0"},{"v":24,"d":"24.0"},{"v":41,"d":"41.0"},{"v":26,"d":"26.0"},{"v":27,"d":"27.0"},{"v":28,"d":"28.0"},{"v":29,"d":"29.0"},{"v":32,"d":"32.0"},{"v":31,"d":"31.0"},0.017,0.005,0.3,0.6]
["2006-11-30T18:04:04",8.9,{"v":24,"d":"24.0"},{"v":41,"d":"41.0"},{"v":26,"d":"26.0"},{"v":27,"d":"27.0"},{"v":28,"d":"28.0"},{"v":29,"d":"29.0"},{"v":32,"d":"32.0"},{"v":31,"d":"31.0"},0.017,0.005,0.4,0.7]