{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Data","Velocity Graph","Pressure Graph"],"not_rendered":{"charts":2,"images":1,"macros":1,"external_links":1,"defined_names":2},"unopened":[{"sheet":"Velocity Graph","index":1,"reason":"not_a_worksheet"},{"sheet":"Pressure Graph","index":2,"reason":"not_a_worksheet"}],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Data","index":0,"n_rows":41,"n_cols":8,"rows_kept":41,"flags":["formulas_cached_only"]}
["Log File Data"]
[]
["2007-05-20T20:43:11","MERIT Configuration Data"]
[]
["Test Description: CERN Testing. Initial Setup."]
[]
["Mode = ****"]
["LogFile = ****"]
["Trigger-Pulse Delay (s) = ****"]
["FlatTop Pct = ****"]
["Jet Accel Time (s) = ****"]
["Jet Steady State Time (s) = ****"]
["Jet Decel Time (s) = ****"]
["Jet SS Velocity (cm/s) = ****"]
["Hg Prefill Vol (liter) = ****"]
["Cylinder Retract Speed (cm/s) = ****"]
["Nozzle Dia (cm) = ****"]
["Hg Volume (liter) = ****"]
["Hg Pressure Alarm (bar) = ****"]
["Hg Temperature Alarm (C) = ****"]
["Hyd Fluid Temp Alarm Level (C) = ****"]
["Hg Cyl Inlet Temp Alarm (C) = ****"]
["Sec Air Temp Alarm (C) = ****"]
["Down Pri Win Temp Alarm (C) = ****"]
["Down Bore Air Temp Alarm (min) (C) = ****"]
["Up Bore Air Temp Alarm (min) (C) = ****"]
["Flange Temp Alarm (C) = ****"]
["Upstream Window Alarm (mbar) = ****"]
["Downstream Window Alarm (mbar) = ****"]
["Hg VaporMonitor 1 Alarm (mg/m^3) = ****"]
["Hg VaporMonitor 2 Alarm (mg/m^3) = ****"]
[]
[]
["Time after Trigger","Nominal Command Signal","Actual Command Signal","Syringe Position","Measured Nozzle Velocity","Hg Pressure","Port A Pressure","Port B Pressure"]
["(ms)","(cm/s)","(cm/s)","(cm)","(cm/s)","(bar)","(bar)","(bar)"]
[0,{"v":0,"d":"0.000"},{"v":0,"d":"0.000"},-19.506,{"v":0,"d":"0.000"},{"v":0,"d":"0.000"},0.879,0.243]
[100,0.054,0.054,-19.506,{"v":0,"d":"0.000"},-0.335,0.728,-0.363]
[200,0.108,0.124,-19.523,{"v":0,"d":"0.000"},-0.108,1.334,1.001]
[300,0.161,0.182,-19.523,{"v":-104,"d":"-104.000"},-0.032,1.031,1.152]
[400,0.215,{"v":0.24,"d":"0.240"},-19.506,{"v":0,"d":"0.000"},-0.184,0.349,{"v":-0.06,"d":"-0.060"}]
[500,0.269,0.321,-19.506,{"v":104,"d":"104.000"},0.044,0.955,1.304]