Issues, 3: Full Turn Extraction

• G10 kicker can deliver beam to A-C lines as well as to U line. • Present power supply sufficient to kick out only 1 bunch. • Upgrade to kick out all 6 bunches requires ≈ 18 months. • Initiate design work in FY99 to complete upgrade in early FY01.