Issues, 5: 70-MHz RF Cavity

• Cavity has 60-cm-diameter iris, 2-m outer diameter.

(Werner Pirkl, CERN) • 4-6 MW peak power to be supplied by four 8973 tubes recommissioned from the LBL Hilac. (Vince LoDestro, BNL; Don Howard, LBL)