Issues, 7: Characterization of Pion Yield

• The final measure of system performance is the capture of soft pions that later decay to muons.

• Add bent solenoid spectrometer downstream of TPC magnet. • Instrument with low-pressure TPC’s and aerogel Čerenkov counters.

• Collect data with slow beam, < 10^6 ppp. • Compare with extrapolations from data of E-910.