Schedule

• FY99:

Prepare A3 area; begin work on liquid jets, extraction upgrade, magnet systems, and rf systems.

• FY00:

Initial beam tests in A3 line. Liquid jet test at NHMFL. (600 hours of AGS beamtime).

• FY01:

Complete extraction upgrade; test of liquid jet + beam. (600 hours).

• FY02:

Complete magnet and rf systems; test with 2 ns beam. (600 hours).

• FY03:

Complete pion detectors; test with low intensity SEB. (600 hours).