AGS Operations Issues

• In FY00/01, HEP operation of AGS is only for the g − 2 experiment, with fast extraction. P951 is very compatible with parasitic running in this condition.

• After FY01, no DOE approved HEP operation of the AGS. • The AGS2000 program proposes running slow extracted proton beam 30-35 weeks/yr, for 16-20 hours/day during RHIC operation.

• P951 requires fast extracted beam, so cannot parasite off the AGS2000 program; we must interleave running with AGS2000, but seek <∼ 6 weeks/yr.

• If there is no other HEP operation of the AGS after FY01, P951 would then bear the full incremental cost of proton beam running.