The Hybrid 20 T Solenoid

Strategy

20 T + r=7.5cm =⇒ P_t ≤ 225 MeV/c Solenoid Attributes • Shielding

– 15 cm ID – 24 cm OD • Inner Coil

– Resistive coil – 4 MW – 6 T – 24 cm ID – 60 cm OD • Outer Coils

– Superconducting – 14 T – 60 cm ID Matching section 20 T → 1.25 T — warm bore 7.5cm → 30cm