The Solenoid Channel

Solenoid outside of rf cavities

ffl Large Warm Bore 200 cm ID ffl Restricted rf cavity radius 100 cm ffl Modest Bz 1.25 T ffl Large Beam Aperture 60 cm ffl Uniform Bz

Solenoids inserted into rf cavities

ffl Reduced Warm Bore 30 cm ID ffl High Bz 5 T ffl Reduced Beam Aperture 30 cm ffl Unrestricted rf cavity radius ffl Non-uniform Bz (Stop bands)