500 MM

55 MM 360 MM 140 MM

40 MM

OUTER VACUUM

SHELL40 K

SHIELD

ALUMINUM SUPPORT

SHELL4 K HE COOLING

TUBE

INNER VACUUM

SHELL

40 K

SHIELD

TEN LAYER

SUPERCONDUCT-

ING COIL

MAGNET SUP-

PORT RING

AXIS OF

ROTATION

SERVICE

PORT REGION FOR COLD

MASS

SUPPORT AND

CRYOSERVICES

LINE OF

SYMME- TRY

LINE OF

SYMME- TRY

CRYOSTAT IR = 300 MM

40 K HELIUM COOLING

TUBE

50 MM

160 MM

CRYOSTAT VACUUM SHELL

SUPPORT RING

70 MM

85 MM

~136 MM