600 MM

HTS LEADS

GAS COOLED

LEADS

CRYOGENIC SER-

VICES PORT

40 K

SHIELD

40 K INTER-

CEPT

40 K HE

4.4 K HE

SUPPORT

RING

~1220 MM

COLD MASS SUP-

PORT

1340 MM