F

F

30 to 50 K Shield

300 K Wall

4.4 K Region

Cold Mass Support Intercept

HTS Leads

In Line Insulator

0.05 g/s 300 K He Gas to Compressor Suction

~2.5 g/s 4.4 K 2-phase He from Previous Magnet

0.05 g/s He Gas at 16 to 30 K from Cold Box

~2.5 g/s 4.2 K 2-phase He to the Next Magnet

Magnet Cooling Tube

Gas Cooled Cu leads

Lead Gas Flow Control