F

F

300 K Cryostat Vacuum Wall

Cold Mass Support Intercept

HTS Leads

0.2 g/s 300 K He Gas to Compressor Suction

10 g/s 4.4 K 2-phase He from Previous Magnet

10 g/s 4.2 K 2-phase He to Next Magnet

31 g/s 16 K He from Cold Box

31 g/s 18 K He to Cold Box to H2 Surge Tank

LH2 Absorber 36 liters

In line Insualtor

Gas Cooled Cu leads

Lead Gas Flow Control

H2 Gas Fill

16 to 40 K Shield

H2 Rupture Disc

S/C Magnet at 4.4 K